# Maintenance Fluids Calculations

## INPUTS

|  |  |
| --- | --- |
| Weight | **Options:** |

## FORMULA

Calculated using the “4-2-1” Rule:

* For 0-10 kg: 4 mL/kg/hr
* For >10-20 kg: 40 mL + 2 mL/kg/hr for every kg >10 kg
* For >20 kg: 60 mL + 1 mL/kg/hr for every kg >20 kg

## FACTS & FIGURES

## EVIDENCE APPRAISAL